**Stokes Bay Tractor Operating Procedures**

The SBSC Launch and Recovery Tractor (with or without a Boat trolley attached) will be limited to travelling at walking pace, ie 3mph in the promenade/ramp area.

Temporary Bollards and warning signs will be positioned across the promenade when launch and recovery movements are being undertaken.

A Banksman wearing a high visibility vest will be present to keep members of the public aware of the vehicle and load movements and associated hazards.

Only SBSC Designated Drivers will drive the SBSC Launch and Recovery Tractor.

SBSC will give training to the banksman

A Flashing light and audible warning will be activated on the Tractor during promenade and ramp movements.

The Figures 1 and 2 shown below are outlines of the proposed Tractor and Boat trolley movements.



Figure 1 Launch movements



Figure 2 Recovery movements